Design ideas:

* Have battery constantly connected to 200 mA power.
* Logic signal from pin 13 activates a (BJT?) switching circuit that enables 600 mA charge.
* Battery load should not vary excessively (investigate to be sure)